REPORTING REQUIREMENTS:	Echo Bay Mines Occurrence 8 Quarry NWB2OCC9799

LICENCE CLASS:	Permit

CONDITIONS APPLYING TO WATER SUPPLY	CONDITIONS APPLYING TO WASTE DISPOSAL

Tailing Containment Area: N7L2 -0925 PART D, ITEM 6

Dewatering quarry occurrence 8 - discharge rate .004-. 006m3 /sec.

Effluent Standards: (100-2)

Parameter	Max. Avg. Conc.	Max. Conc. Grab.

Total Arsenic	0.5 mg/l	1.00 mg/l

Total Copper	0.15 mg/l	0.30 mg/l

Total Lead	0.10 mg/l	0.20 mg/l

Total Nickel	0.20 mg/l	0.40 mg/l

Total Zinc	0.40 mg/l	0.80 mg/l

Suspended Solids	15 mg/l	30 mg/l

pH	6.0 - 9.5

DESCRIPTION	FEB.	MARCH	APRIL	MAY	JUNE	JULY	AUGUST	SEPT.	OCT.	NOV.	DEC.
EFFECTIVE DATE	1,1997
EXPIRY DATE	31,1999
PART B
1.	Annual water use fee	Received
2.	Annual Report	Due	31,Yearly
Received	02,1998
3.	Spill Reported	Hotline
Inspector
4.	Notification of Modification	Planned
Completed
PART C
3.	Discharge rate	Received	6,1997A
5.	Notification change in operation	Planned
Received
Approved
6.	Within effluent qty limits	Performed	1,1997B
7.	Notification of discharge	Received
Planned
Inspector
PART D
6.	Lab approved by Board	Received
SNP
1.	Monthly SNP Report	Received	2/25/98	4/31/98	5/8/98	6/23/98	20,98	28,98	11/18/98
AMENDMENTS:
1.	Discharge rate Increased	6,1997A
INSPECTION REPORT DIAND

COMPLIANCE REPORT DIAND

Rate increased to . 018m3 /sec

All waste water discharge from OCC 8 quarry shall meet the following effluent quality requirements at station 100-2: