REPORTING REQUIREMENTS:	Lytton Minerals Limited. Jericho Diamond N7L2 -1666

LICENCE CLASS: B

CONDITIONS APPLYING TO WATER SUPPLY	CONDITIONS APPLYING TO WASTE DISPOSAL

Water Supply: Carat Lake	Tailing Containment Area:

Daily quantity not to exceed 25 cubic metres.	Minewater Collection Sys.:

Effluent Standards:

Parameter	Max. Avg. Conc.	Max. Conc. Grab.

Total Arsenic	0.50 mg/l	1.00 mg/l

Total Copper	0.30 mg/l	0.60 mg/l

Total Lead	0.20 mg/l	0.40 mg/l

Total Nickel	0.50 mg/l	1.00 mg/l

Total Zinc	0.50 mg/l	1.00 mg/l

Suspended Solids	25.0 mg/l	50.0 mg/l

Oil and Grease	5.0 mg/l

pH	6.0 - 9.5

Sewage Disposal:

Effluent Standards:

Parameter	Max. Avg. Conc.

Fecal Coliform	1000 CFU /100 ml

Oil and Grease	5.0 mg/l

Total Suspended Solids	35.0 mg/l

BOD	30.0 mg/l

pH	6.0-9.5

DESCRIPTION	FEB.	MARCH	APRIL	MAY	JUNE	JULY	AUGUST	SEPT.	OCT.	NOV.	DEC.
EFFECTIVE DATE	1, 1996
EXPIRY DATE	30, 1998
Annual water use fee
PART B
1.	Security Deposit $ 50,000.00

2.	Annual Report	Due	31, Yearly
Received
PART C
3.	Notification of Discharge	Received
Planned
PART D
1.	Notification of Modification	Planned
Completed
9.	Inspection and follow-up Plan	Due
PART E
1.	Contingency Plan	Due
3.b	Spill Reported	Hot Line
Inspector
SNP
1.	Monthly SNP Report	Received	16,1997	03,1998
9.	QA /QC Plan	Due
Recieved
Approved
INSPECTION REPORT DIAND

COMPLIANCE REPORT DIAND

Comments:

Inspection not done in 1997, UPDATE THIS FILE, STILLS NEED TO BE DONE.

Revisions: