REPORTING REQUIREMENTS:	Cumberland Resources - NWB2ATU9899

LICENCE CLASS: Water use and waste disposal

associated with Exploratory Drilling

CONDITIONS APPLYING TO WATER SUPPLY	CONDITIONS APPLYING TO WASTE DISPOSAL

Water Supply: Atulik Lake	Tailing Containment Area:

Daily quantity not to exceed 100 cubic metres.	Minewater Collection Sys.:

Effluent Standards:

Parameter	Max. Avg. Conc.	Max. Conc. Grab.

Total Arsenic	0.30 mg/l	0.60 mg/l

Total Copper	0.20 mg/l	0.40 mg/l

Total Cyanide	0.80 mg/l	1.60 mg/l

Total Lead	0.20 mg/l	0.40 mg/l

Total Nickel	0.30 mg/l	0.60 mg/l

Total Zinc	0.30 mg/l	0.60 mg/l

Suspended Solids	25 mg/l	50 mg/l

pH	6.0 - 9.5

Sewage Disposal:

Effluent Standards:

Parameter	Max. Avg. Conc.	Max. Conc. Grab.

Fecal Coliform	CFU / dL

BOD	mg/l

Total Suspended Solids	mg/l

Oil and Grease	mg/l

pH	6.0-9.5

DESCRIPTION	FEB.	MARCH	APRIL	MAY	JUNE	JULY	AUGUST	SEPT.	OCT.	NOV.	DEC.
EFFECTIVE DATE	22, 1998
EXPIRY DATE	31, 1999
PART B
2.	Security Deposit
1.	Annual Water Use Fee
5.	Annual Report	Due	31, Yearly
Received
PART C
Due
Received
PART D
4.	Notification of Discharge	Received
Planned
9.	Inspection and follow-up Plan	Due
9.	Inspection and follow-up Plan	Received
Approved
10.	Annual Geotechnical Inspection	Performed
Engineer's Report	Due
Received
PART E
1.	Contingency Plan	Due
3.b	Spill Reported	Hot Line
Inspector
PART F
1.	Notification of Modification	Planned
Completed
3	As- builts submitted 60 days after completion
PART H
1.	A&R Plan	Due
Received
Approved
3.	Estimate of RECLAIM	Due
Received
7.	NOTIFICATION CLOSURE	Planned
8.	FINAL A&R PLAN	Received
SNP
1.	Monthly SNP Report	Received
2.	QA /QC Plan	Due
Recieved
AMENDMENTS:
1.
INSPECTION REPORT DIAND

COMPLIANCE REPORT DIAND

Comments:

Revisions: