1)	Coordinate upgrade of main service with NWTPC and install of new service feeders, meter base, enclosed circuit breakers and splitters in shower building. Pay for all utility costs from a power cash allowance of $10,000.

2)	Supply and install electrical services via underground service cables c/w trenching, backfilling and compacting from shower building to two new power panels (P.P. #1 and P.P. #2) and to one existing power panel (P.P #3) from which will run underground electrical service cables to provide power to the 21 out of 32 individual campground sites.

3)	a)	Supply and install two Power Panels (P.P. #1 and P.P. #2) and associated backboard and cable reduction splitter box which will supply campsites with combined 30/15 Amp service.

b)	Power panels #1 and #2 will be Nema 4 weather proof metal/lockable panels, each containing a 100 Amp 24-circuit panel.

c)	Power Panel #3 (P.P. #3) existing panel will be weather proof metal/lockable panels, containing a 60 Amp 24-circuit panel. This breaker must be replaced with a 100Amp breaker. Panel is to be re-installed at higher height as shown on drawings along with new backboard and cable reduction splitter box.

d)	Power Panel #1 (P.P. #1) will feed eight campsites (#1, #2, #3, #4, #5, #6, #19, #20) which will each require:

1 - 30 amp - 125 volt 1 pole 3-wire (includes ground) TT-30R Receptacle (see item #3)

1 - 15 amp - 115 volt duplex receptacle (see item #3)

e)	Power Panel #2 (P.P. #2) will feed six campsites (#7, #8, #9, #10, #11, #12) which each will require:

1 - 30 amp - 125 volt 1 pole 3-wire (includes ground) TT-30R Receptacle (see item #3)

1 -15 amp - 115 volt duplex receptacle (see item #3)

f)	Power Panel #1 (P.P. #3) will feed seven campsites (#13, #14, #15, #16, #17, #18, #32) which will each require:

1 - 30 amp - 125 volt 1 pole 3-wire (includes ground) TT-30R Receptacle (see item #3)

1 - 15 amp - 115 volt duplex receptacle (see item #3)

Note: #15,#17 & #32 only require one new 30 amp receptacle, remove and replace existing 15 amp receptacle feeders and re-use existing pedestals at these sites.

g)	Supply and install electrical services via underground service cables c/w trenching, backfilling and compacting from P.P #1 to gate house and from P.P #2 to Kitchen Shelter.

4)	Supply and install 21 exterior parking power outlet boxes of which all 21 will be Model #FS - boxes with weatherproof metal covers made by Iberville. The boxes will be for installation as shown on drawing E-05. The outlet boxes will be mounted onto the side of the 6"x6" pressure treated wooden posts.

5)	To supply and install 27 exterior 6"x6" PWF treated wooden posts. The 6"x6" PWF treated posts will be 2350 mm (7.7 ft.) long, of which 950 mm (3.1 ft.) will be below ground.

6)	Paint 6" x 6" posts "Parks Grey" with paint supplied by GNWT-PWS. Posts to be painted minimum of 6" below grade.

Note #1	The contractor will be responsible for confirming all site dimensions and routes for all under ground cables, cable trenching requirements from the shower building to the power pedestals and to the individual campsites. The attached distances and routes are to be used only as a guide.

Note #2	All work will be done in accordance to the current applicable codes governing the work.

Note #3	Cable shall be sleeved in PVC conduit.