REPORTING REQUIREMENTS:	Echo Bay Mines Ltd - NWB2ULU9700

LICENCE CLASS:	Advanced Exploration

CONDITIONS APPLYING TO WATER SUPPLY	CONDITIONS APPLYING TO WASTE DISPOSAL

Water Supply:	West Lake ~ 100 cubic metres/ day	Sewage Treatment: RBC Unit

Sludge removed to lined depression under waste rock pad

Sewage Disposal Effluent Standards:

Parameter	Max. Avg. Conc.	Max. Conc. Grab.

Total Arsenic	0.50 mg/L	1.00 mg/L

Total Copper	0.30 mg/L	0.60 mg/L

Total Lead	0.20 mg/L	0.40 mg/L

Total Zinc	0.50 mg/L	1.00 mg/L

Total nickel	0.50 mg/L	1.00 mg/L

Oil and Grease	5.0 mg/L

Suspended Solids	25 mg/L	50 mg/L

pH	6.0-9.5

DESCRIPTION	FEB.	MARCH	APRIL	MAY	JUNE	JULY	AUGUST	SEPT.	OCT.	NOV.	DEC.
EFFECTIVE DATE	1, 1997
EXPIRY DATE	31, 2000
PART B
1.	Annual Water Use Fee	08,99C
2.	Security Deposit
a) $250,000.00
5.	Annual Report	Due	31, Yearly
Received
PART D
INSPECTION REPORT DIAND

16,1997B BB
COMPLIANCE REPORT DIAND

Comments:

A	Application filed with the NWB currently drafting licence. Notification camp temporary closure due to gold $.

B	Overview of the operation provided. No significant concerns.

C	Water use fees received Feb 8, 99 covers up to Nov 30, 99.